**EMISOR RMC166CHS**

**INSTRUCCIONES DE PROGRAMACIÓN**

- El emisor RMC166CHS sólo puede ser programado con las programadoras Remocon HCD900 y HCD900-Q por un profesional. Diríjase a un distribuidor autorizado para programar su mando.

- De manera alternativa el emisor RMC166CHS puede unificar hasta cuatro mandos de código evolutivo y / o código fijo de frecuencia 433.92 MHz. Cada pulsador del emisor RMC166CHS puede emitir un código diferente.

**UTILIZACIÓN**

- Pulse el botón correspondiente al canal de activación del receptor dentro del radio de acción del mismo.

**SUSTITUCIÓN DE LA PILA**

- Abra el emisor RMC166CHS con la ayuda de un destornillador de estrella pequeño. Retire la pila agotada y reemplácela por una pila alcalina de 12V del tipo 23A respetando siempre las polaridades marcadas en el emisor. Deposite la pila usada en un recipiente adecuado para su reciclado.

**DECLARACIÓN DE CONFORMIDAD**

El que suscribe José Martín Tejero; Remocon Spain S.L.; C/ Ignacio Aldecoa, 15, 29004 Málaga. Declara bajo su responsabilidad que el emisor RMC166CHS cumple con lo dispuesto en la Directiva 2014/53/EU y 2014/35/EU del Parlamento Europeo.

**RADIO : EN 300 220-1: V3.1.1 (2017-02) EN 300 220-2: V3.1.1 (2017-02)**

**EMC : EN 301 489-1: V2.2.3 (2019-11) EN 301 489-3: V2.1.1 (2019-03)**

**SEGURIDAD : EN 62368-1:2014/A11:2017 IEC 62368-1:214/COR1:2015**

|  |  |
| --- | --- |
| **FRECUENCIA** | **433.92 MHZ** |
| **CÓDIGO** | **EVOLUTIVO + FIJO** |
| **VERSIÓN** | **4 PULSADORES** |
| **ALCANCE** | **50 METROS** |
| **ALIMENTACIÓN** | **12V** |

**RMC166CHS TRANSMITTER**

**PROGRAMMING INSTRUCTIONS**

- The RMC166CHS transmitter can only be programmed by a professional with the HCD900 or HCD900-Q duplicators. Please go to a Remocon Official Distributor to buy your transmitter.

- The RMC166CHS transmitter is able to unify up to four different fixed and / or rolling code transmitters. Every button of the RMC166CHS transmitter is able to emit a different code.

**USAGE**

- Press the corresponding button to activate the desired channel on the receiver inside its operational range.

**REPLACING THE BATTERY**

- Open the RMC166CHS transmitter using a small screwdriver and replace the battery with a 12V 23A alkaline battery only maintaining the polarity marked on the case. Dispose off of the used battery properly.

**CONFORMITY DECLARATION**

The undersigned Jose Martin Tejero; Remocon Spain S.L.; C/ Ignacio Aldecoa 15, 29004 Malaga, declares under his responsibility that the RMC166CHS transmitter conforms to the directive and standards 2014/53/EU and 2014/35/EU from the European Parliament.

**RADIO : EN 300 220-1: V3.1.1 (2017-02) EN 300 220-2: V3.1.1 (2017-02)**

**EMC : EN 301 489-1: V2.2.3 (2019-11) EN 301 489-3: V2.1.1 (2019-03)**

**SAFETY : EN 62368-1:2014/A11:2017 IEC 62368-1:214/COR1:2015**

|  |  |
| --- | --- |
| **FREQUENCY** | **433.92 MHZ** |
| **CODE** | **ROLLING + FIXED CODE** |
| **VERSION** | **4 BUTTONS** |
| **OPERATIONAL RANGE** | **50 METERS** |
| **VOLTAGE** | **12V** |